**Product Name: Metal Access Panel**

**Product Code: BYMAPPW**

**General Schematic**



**Definitions**

Neck size: Nominally cited in listing title. Size of the opening that would be cut into the wall/ceiling to install the access panel. Depicted via N1, N2 in schematic

Opening size: Size of opening available for access once panel is installed. Depicted via W1, L1

Overall size: Total size of access panel as visible once installed. Depicted via W2, L2

**Size chart**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Product number** | **Nominal size****(in).** | **Nominal size****(mm)** | **Neck size****N1XN2****(mm)** | **Opening size****W1XL1****(mm)** | **Overall size****W2XL2****(mm)** |
| BYMAPPW-0606 | 6X6 | 150X150 | 147X147 | 145X145 | 185x185 |
| BYMAPPW-0808 | 8X8 | 200X200 | 197X197 | 195X195 | 235x235 |
| BYMAPPW-1212 | 12X12 | 300X300 | 297X297 | 295X295 | 335x335 |
| BYMAPPW-1216 | 12X16 | 300X400 | 297X397 | 295X395 | 336x436 |
| BYMAPPW-1220 | 12X20 | 300X500 | 297X497 | 295X495 | 336X536 |
| BYMAPPW-1616 | 16X16 | 400X400 | 397X397 | 395X395 | 435x435 |
| BYMAPPW-1620 | 16X20 | 400X500 | 397X497 | 395X495 | 436x536 |
| BYMAPPW-1624 | 16X24 | 400X600 | 397X597 | 395X595 | 436X636 |
| BYMAPPW-1818 | 18X18 | 450X450 | 447X447 | 445X445 | 485X485 |
| BYMAPPW-2020 | 20X20 | 500X500 | 497X497 | 495X495 | 536x536 |
| BYMAPPW-2024 | 20X24 | 500X600 | 497X597 | 495X595 | 536X636 |
| BYMAPPW-2424 | 24X24 | 600X600 | 597X597 | 595X595 | 636X636 |

**Other specifications:**

* 1mm galvanized steel frame and lid
* Flange frame
	+ Sizes up to 18”x18” with one piece punched frame
	+ 20”x20” and larger with welded frame
* White powder coating finish
* High durability and corrosion protection
* Steel bar hinge door removable
* Swing tabs for installation of fixing screws
* Two push locks. Push on centre-right of door to open / close
* Packaging: Each piece put into poly bag with shrink wrap, wrapped with foam around edges, then put into carton
* Made in China