{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["WMS,A Given"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"WMS,A Given","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[[17,0,17,1],[19,0,19,1],[8,4,8,6],[21,2,21,10],[17,2,17,4],[19,2,20,9],[5,4,5,6],[0,0,0,1],[7,0,7,1],[3,7,4,10],[3,4,3,5],[2,3,2,5],[7,4,7,6],[4,4,4,5],[6,0,6,1]]}
["Given"]
["WMS",75.375]
["A",25.25,null,"A = (WMS/2) - PinionOffset"]
["Locker Gap",0.188,null,0.188,"for 45 Spline Spools",null,null,"Spider 9 Rear Housing & Shaft Calculator for PRO SERIES UNIT BEARINGS"]
["Pinion to Locker",2.75,null,0.5,"for 35/40 Spline Spools"]
[null,null,null,1.5,"for 35/40 Spline ARB Air Lockers",null,null,null,null,null,{"$f":"TODAY()","v":"2023-03-21"}]
["Solved for"]
["Pro Series Unit Bearings",null,null,2.125,"for 35/40 Spline ARB Air Lockers"]
["B",{"$f":"B2-B3","v":50.125},null,2.75,"for 45 Spline GearWorks Spools"]
["Ta",{"$f":"CEILING(B3-3.95875-4,1/16)","v":17.3125}]
["Tb",{"$f":"CEILING(B9-3.95875-6,1/16)","v":40.1875}]
["Pa",{"$f":"B10+4","v":21.3125}]
["Pb",{"$f":"B11+6","v":46.1875}]
["Sa",{"$f":"CEILING(3.49575+$B$10+4+$B$5-($B$4/2),1/16)","v":27.5}]
["Sb",{"$f":"CEILING(3.49575+$B$11+6-$B$5-($B$4/2),1/16)","v":46.875}]
["Pinion Offset",{"$f":"(B3-B9)/2","v":-12.4375}]
[]
["Pinion Offset:",null,"+ Passenger / - Driver"]
[]
["Components Used:",null,"Spider 9 Housing, Pro Series Unit Bearings, Spidertrax Brake Hats, 9\"/10\" Differential (High or Low Pinion)"]
[]
[null,null,"Questions, please contact us at support@spidertrax.com or (303) 772-0033."]